NAME
  primary - get or set primary components

SYNOPSIS
  primary TYPE
  primary TYPE ADDRESS

DESCRIPTION
  This program allows reading the address of the current primary component of the specified type. It also allows changing the current primary component for a specified type by providing the (abbreviated) address of the new primary component.

EXAMPLES
  primary gpu
    Writes the address of the current primary GPU to the standard output.

  primary gpu 24a
    Makes the GPU of which the address starts with `24a` the new primary GPU.